Offline Data Back up

START

IF there is a Data Stored

IS there connection to cloud

TRUE FALSE

FALSE TRUE

Complete Data will be enqueue in SD Card

Resume Data Gathering operation

IF Data has been sent

Digital Data will be send to Microcontroller

Data Stored in the SD CARD will be read

TRUE FALSE

The Data will be dequeue